{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"merged":[[0,0,0,8],[2,0,8,0],[13,0,15,0],[17,0,27,0],[21,1,23,1],[21,2,23,2],[21,8,23,8],[24,1,27,1],[24,2,27,2],[24,8,27,8],[28,0,28,1],[28,2,28,6]],"flags":["formulas_cached_only"]}
["2016年部分零星维修材采购清单"]
["包号","序号","品    名","投标规格","数量","单位","单价（元）","小计（元）","投标备注"]
["第一包：水材料",1,"红外线感应节水器与电子阀",null,20,"套",null,null,"本品可与用户单位原有节水器所有零部件通用互换"]
[null,2,"MN型自动冲水芯  ",null,10,"只",null,null,"本品可与用户单位原有节水器所有零部件通用互换"]
[null,3,"纯铜快开加长水龙头 ","型号：φ20",100,"只"]
[null,4,"全铜双联面盆水嘴",null,10,"只"]
[null,5,"三角阀","型号：φ15",50,"只",null,null,"全铜"]
[null,6,"不锈钢软管     ","型号：60cm ",50,"根"]
[null,7,"镀锌铸铁盖帽   ","型号：φ20",100,"个",null,null," 本品可与用户单位原有节水器所有零部件通用互换"]
[null,8,"生料带",null,100,"卷"]
[null,9,"延时阀和延时阀弯头","拆下两边螺帽体长7cm",30,"套",null,null,"纯铜"]
[null,10,"延时阀和延时阀弯头","拆下两边螺帽体长8cm",30,"套",null,null,"纯铜"]
[null,11,"PVC落水箱",null,20,"只",null,null,"本品可与用户单位原有节水器所有零部件通用互换"]
["第二项、电材料",1,"楼顶扇 ","型号：FSLD-40",80,"台",null,null,"品牌：格力，可与用户单位原有楼顶扇所有零部件通用互换"]
[null,2,"楼顶扇涡轮/摇头齿轮箱","配套品牌：格力，型号：FSLD-40，需要用户单位原有楼顶扇所有零部件通用互换",50,"个"]
[null,3,"BV2.5单股铜芯线","1卷=100M",6,"卷",null,null,"需分色"]
[null,4,"86型五眼插座",null,80,"个",null,null,"品牌：正泰、公牛、德力西"]
[null,1,"五合板       ","2440*1220*5mm",10,"张",null,null,"板纹路与用户单位学生公寓内家具纹路类似"]
[null,2,"三合板      ","2440*1220*3mm",10,"张"]
[null,3,"密度板       ","2440*1220*18mm",10,"张"]
[null,4,"收边条      ","PVC材质；宽1.8mm",50,"根",null,null,"颜色与用户单位学生公寓内家具颜色类似"]
[null,4,"铰链","全盖式    ",80,"付"]
[{"$nulls":3},"半盖式    ",80,"付"]
[{"$nulls":3},"内嵌式    ",80,"付"]
[null,6,"轨道","三截式    ",30,"付"]
[{"$nulls":3},"35cm      ",30,"付"]
[{"$nulls":3},"40cm      ",30,"付"]
[{"$nulls":3},"45cm      ",30,"付"]
["总 计："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}